
1. OZR 202 HOSPITAL BED (PLASTIC SIDE RAIL)
1. 
1. 
1. 
1. • Electrical operated backrest and  legrest movement.
[bookmark: _Hlk242690629]             • Patient handset.
1. • Retracting backrest for advanced comfort, less pressure.
1. • Hygienic design (PP), lockable and tuck away side rails 
1. • Easy adjustable knee break position.
1. • Removable head and foot boards.
1. • 125 mm directional lock castors.
1. • Electrostatic painted metal frame.
1. • Metal sheet sleep surface
1. • Height adjustable  IV pole.
	
TECHNICAL SPECIFICATIONS

Overall Dimesions: (Max.)
	



105 – 216 cm

	Footrest Angle (Max.)
	0° – 35°

	Height range without Mattress
	42 -78  cm

	Trendelenburg                                          
	12°     

	Reverse  Rrendelenburg                          
	12°     

	Mattress Platform (ABS)
	90 x 200 cm

	Castor Diameter
	12,5 cm 

	Safe Working Load
	220 kg
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