






   OZR 4004N ICU BED


• Electrical operated backrest,  legrest and high/low adjustment.
• Trendelenburg and reverse trendelenburg adjustments electrical operated
[bookmark: _Hlk242690629]• Patient handset.
•Nurse Control Unit(optional)
• Retracting backrest for advanced comfort, less pressure.
• Auto contour.
• Hygienic design (PP), lockable and tuck away side rails with angle indicator
• Easy adjustable knee break position.
• Removable head and foot boards.
• 125 mm directional lock castors.(cenral lock optional)
• Electrostatic painted metal frame.
• Compact HPL sleep surface
• Height adjustable  IV pole.

	
TECHNICAL SPECIFICATIONS

Overall Dimesions: (Max.)
	



105 – 216 cm

	Footrest Angle (Max.)
	0° – 75°

	Height range without Mattress
	42 -82  cm

	Trendelenburg                                          
	16°     

	Reverse  Rrendelenburg                          
	16°     

	Mattress Platform (ABS)
	90 x 200 cm

	Castor Diameter
	12,5 cm 

	Safe Working Load
	225 kg

	Power In
	230V, 50HZ





