



   OZR 5005 HOSPITAL BED WITH COLOUMN


• Electrical operated backrest,  legrest and high/low adjustment.
• Trendelenburg and reverse trendelenburg adjustments electrical operated by coloumn motors.
[bookmark: _Hlk242690629]• Patient handset.
•Nurse Control Unit
• Retracting backrest for advanced comfort, less pressure.
• Auto contour.
• Hygienic design (PP), lockable and tuck away side rails with angle indicator
• Easy adjustable knee break position.
• Removable head and foot boards.
• 150 mm Central lock castors.(150 twin castors are optinal)
• Electrostatic painted metal frame.
• Compact HPL sleep surface
• Height adjustable  IV pole.
• High density Mattress



	
TECHNICAL SPECIFICATIONS

Overall Dimesions: (Max.)
	



105 – 216 cm

	Footrest Angle (Max.)
	0° – 35°

	Height range without Mattress
	45 -78  cm

	Trendelenburg                                          
	12°     

	Reverse  Rrendelenburg                          
	12°     

	Mattress Platform (ABS)
	86 x 195 cm

	Castor Diameter
	12,5 cm 

	Safe Working Load
	250 kg

	Power In
	230V, 50HZ
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