




OZR PLUS MNL3 MANUAL HOSPITAL BED 



• Backrest movement with mechanical crank. 
• Hygenical design metal collapsible siderails
• Hygenical design plastic easily removable head and foot boards.
•360° rotating cross brake system
• 125 mm directional lock castors.
• Electrostatic powder painted metal frame.
• Metal sheet sleep surface
• Height adjustable  IV pole.
• Accessories space on 4 corners .


	
TECHNICAL SPECIFICATIONS

Overall Dimesions: (Max.)
	



90 – 200 cm

	Height range without Mattress
	45 cm

	Mattress Platform (ABS)
	86 x 195 cm

	Castor Diameter
	12,5 cm 

	Safe Working Load
	225 kg








